


CHANGE TO CONTRACT NOTICE (CHANGE NOTICE)

2.1. General information  
Information about previous notices:
Contract Notice Title: Supply, Delivery, Installation, Commissioning and Training for One (1) Mobile Jaw Crusher Machine with an Integrated Picking Station for the Re-use and Management of Construction and Demolition Waste

Contract Notice Reference Number (procedure identifier): RE-CONSTRUCT/IPA/2026/SUP/T01
[bookmark: OLE_LINK3]10. Change
Main reason for change: 
Modification of original information submitted by the contracting authority.
Description: Modifications based on the clarification requests received by prospective tenderers
All the changes described below are reflected in the respective documents. The corrigendum package “RE-CONSTRUCT/IPA/2026/SUP/T01Corrigendum 1” contains all the revised documents:
- TD1 RC Annex_SAT_and_EAR_rev 1
- TD1 RC c4f_annexiitechspeciiitechoffer_en_rev 1
- TD1 RC c4b_itt_en_rev 1
- TD1 RC Clarifications to the questions
And can be downloaded here: https://skopje.gov.mk/media/12225/re-construct_ipa_2026_sup_t01-corrigendum-1.zip

In case of differences with the original documents, the revised version prevails and it is considered valid.

10.1. Text to be corrected in the original notice

Section No5.1.12. Terms of procurement

Instead of:Deadline for submission of tenders: 
Date: 30.09.2026 
Local Time: 14:00

Read:Deadline for submission of tenders: 
Date: 22.10.2026 
Local Time: 14:00

10.2. Modifications to other tender documents
Document:TD1 RC c4f_annexiitechspeciiitechoffer_en  “ANNEX II + III: TECHNICAL SPECIFICATIONS + TECHNICAL OFFER”  (Revised version attached)
Section No 1.1
Instead of: Capacity of processing: 
- min 50 t/Hour up to 250 t/hour
Read: Capacity of processing:   
- min 100 t/Hour up to 250 t/hour
Capacity of processing: Manufacturer-declared nominal processing capacity of at least 100 t/h. Equipment with a higher nominal processing capacity is acceptable.

Section No 1.3
Instead of: Drive unit: 
- Diesel engine
Read: Drive unit: 
- Diesel engine or dual-power diesel-electric configuration.Integrated diesel engine, or dual-power diesel-electric configuration, provided that the machine can perform all required functions and achieve the required processing capacity independently using its integrated diesel-powered system. Connection to an external electricity supply shall be optional and shall not be required for normal operation or SAT.

Section No 1.5
Instead of: Input technology and size capacity:
-Integrated picking station i.e. vibrating frame for receiving CDW 120mm - 250mm
Read: Input technology and size capacity:
· The machine shall be capable of accepting incoming construction and demolition waste with a manufacturer-declared maximum permissible feed size of at least 500 mm.
· The machine shall be equipped with an integrated receiving hopper with a vibrating feeder and a minimum hopper capacity of 3.5 m³.
· No separate manual picking station, picking conveyor or personnel picking platform is required.
· The required integrated magnetic separator for metals is specified separately under Annex II item 1.9..

Section No 1.6
Instead of: Output granulation capacity: Adjustable from 10mm-40mm 
Read: Crusher discharge/CSS setting: Adjustable from 10mm-200mm

Section No 1.7
Instead of: Mobility:
		- Independent movement of rubber tracks driven by hydraulic drive; or
- Forced propulsion with integrated tow-bar, axles and wheels
Read: Mobility:
		- Self-propelled tracked machine

Section No **1.15 Delivery and Installation, subsection 5.1 Mechanical Inspection and Commissioning:

Instead of: 
		- Assembly and installation of the crusher and integrated picking station

Read: 
- Assembly and installation of the crusher, integrated receiving hopper and vibrating feeder

Section No **1.15 Delivery and Installation, subsection 5.5 Performance Testing and Site Acceptance Test (SAT): 

Instead of: 
- Verifying operation of: -integrated picking station;

Read: 
- Verifying operation of: -integrated receiving hopper and vibrating feeder;


Document :TD1 RC c4b_itt_en(Revised version attached)
Section 2. Timetable
Instead of: 
	
	DATE
	TIME**

	Information meeting / site visit (if any)
	Not applicable
	Not applicable

	Deadline for requesting clarifications from the contracting authority
	09.09.2026
	14:00

	Last date on which clarifications are issued by the contracting authority
	22.09.2026
	-

	Deadline for submission of tenders
	30.09.2026
	14:00

	Tender opening session
	02.10.2026*
	

	Notification of award to the successful tenderer
	30.10.2026*
	-

	Signature of the contract
	November 2026 *
	-



Read:
	
	DATE
	TIME**

	Information meeting / site visit (if any)
	Not applicable
	Not applicable

	Deadline for requesting clarifications from the contracting authority
	09.09.2026
	14:00

	Last date on which clarifications are issued by the contracting authority
	22.09.2026
	-

	Deadline for submission of tenders
	22.10.2026
	14:00

	Tender opening session
	26.10.2026*
	

	Notification of award to the successful tenderer
	30.11.2026*
	-

	Signature of the contract
	December 2026 *
	-



Section No 10.4, paragraph 2
Instead of: The technical and financial offers must be placed together in a sealed envelope. The envelope should then be placed in another single sealed envelope/package, unless their volume requires a separate submission for each lot.]

Read: The technical and financial offers must be placed in a separate sealed envelope each. These envelopes should then be placed in another single sealed envelope/package, unless their volume requires a separate submission for each lot.


Document :TD1 RC Annex_SAT_and_EAR(Revised version attached)
Multiple content revision, new version released

Instead of version: TD1 RC Annex_SAT_and_EAR, 
New valid version: TD1 RC Annex_SAT_and_EAR_ver1 (attached)

[bookmark: _Toc42488071]All other terms and conditions of the contract notice remain unchanged. The above alterations and/or corrections to the contract notice are integral part of the contract notice.
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